|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Cuckfield Parish Council: Courtmead Road Drainage Improvements** | | | | |
| **Description** | **Quantity** | **Unit** | **Rate £** | **Total £** |
| Preliminaries, Mobilisation, Insurances, Pedestrian and Traffic Management - Chapter 8 signage and 2-way traffic lights as required.  To be read in conjunction with the Cuckfield Scope Plan. |  |  |  |  |
| **Courtmead Road Drainage Improvements** |  |  |  |  |
| Install new pipeline - 225mm Upvc twinwall pipe with ST1 concrete bed and surround including. tarmac reinstatement to HAUC specification | 65 | Lin M |  |  |
| Install new pipeline - 225mm Upvc twinwall pipe with ST1 concrete bed and surround including reinstatement with topsoil and grass seed | 90 | Lin M |  |  |
| Excavate for and install new 1050mm diameter catchpit manhole in carriageway. Catchpit to have minimum 450mm sump below outgoing inverts. | 2 | number |  |  |
| **For the TOTAL sum of (excluding VAT)** |  |  |  |  |
| **Grand Total** **sum of (excluding VAT)** |  |  |  |  |
| *Notes: No allowance for Highways Licenses fees* |  |  |  |  |